DICOM PS3.3 2020d - Information Object Definitions

A.5.4 NM Image IOD Module Table (Current)
Prev | A.5 Nuclear Medicine Image IOD | Next

### A.5.4 NM Image IOD Module Table

Table A.5-1 specifies the Modules of the NM Image IOD.

Table A.5-1. NM Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
NM/PET Patient Orientation | C.8.4.6 | M
Frame of Reference | Frame of Reference | C.7.4.1 | U
Synchronization | C.7.4.2 | C - Required if time synchronization was applied
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Acquisition Context | C.7.6.14 | U - See Section A.5.4.1
Device | C.7.6.12 | U
Specimen | C.7.6.22 | U
NM Image Pixel | C.8.4.7 | M
Multi-frame | C.7.6.6 | M
NM Multi-frame | C.8.4.8 | M
NM Image | C.8.4.9 | M
NM Isotope | C.8.4.10 | M
NM Detector | C.8.4.11 | M
NM TOMO Acquisition | C.8.4.12 | C - Required if Image Type (0008,0008) Value 3 is TOMO, GATED TOMO, RECON TOMO or RECON GATED TOMO
NM Multi-gated Acquisition | C.8.4.13 | C - Required if Image Type (0008,0008) Value 3 is GATED, GATED TOMO, or RECON GATED TOMO
NM Phase | C.8.4.14 | C - Required if Image Type (0008,0008) Value 3 is DYNAMIC
NM Reconstruction | C.8.4.15 | C - Required if Image Type (0008,0008) Value 3 is RECON TOMO or RECON GATED TOMO
Overlay Plane | C.9.2 | U
Multi-frame Overlay | C.9.3 | U
VOI LUT | C.11.2 | U
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

### Note

The Curve Module (Retired) was previously included in the Image IE for this IOD but has been retired. See PS3.3-2004.

#### A.5.4.1 Acquisition Context Module

For Acquisition Context Sequence (0040,0555) DTID 3470 “NM/PET Acquisition Context” shall be used, which includes description of the cardiovascular rest or stress state.

The Acquisition Context Sequence (0040,0555) shall always apply to all frames in the Image. Patient State shall always apply to all frames in the Image, therefore, neither Referenced Frame Numbers (0040,A136) nor Referenced Frame Number (0008,1160) shall be present.

The Acquisition Context information may be entered during acquisition, or obtained from the Modality Worklist using information supplied in the Protocol Context, using TID 15101 “NM/PET Protocol Context”.

Prev | Up | Next
A.5.3 NM Image IOD Module Table (Retired) | Home | A.6 Ultrasound Image IOD

DICOM PS3.3 2020d - Information Object Definitions