DICOM PS3.17 2020d - Explanatory Information

XXX.3.9.3 Encoding Details (Current)
Prev | XXX.3.9 Stent Stabilization | Next

#### XXX.3.9.3 Encoding Details

##### XXX.3.9.3.1 Volumetric Presentation State Identification Module Recommendations

Table XXX.3.9-1. Volumetric Presentation State Identification Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Presentation Sequence Collection UID | (0070,1102) | Set to the same UID value in each of the Presentation State instances indicating the views are sequentially ordered.
Presentation Sequence Position Index | (0070,1103) | Set to "1" for first phase, "2" for second phase, etc.

Prev | Up | Next
XXX.3.9.2 Encoding Outline | Home | XXX.3.9.3.2 Volumetric Presentation State Relationship Module Recommendations

DICOM PS3.17 2020d - Explanatory Information