DICOM PS3.4 2020d - Service Class Specifications

FF.2.3.2 Description of Display Components (Current)
Prev | FF.2.3 Volumetric Presentation State Display | Next

#### FF.2.3.2 Description of Display Components

##### FF.2.3.2.1 Classification Component Components

There are two classification component types currently defined for conversion from scalar input data to RGBA. The defined components are:

- One Input -> RGBA: This component accepts reconstructed data from one input in the Volumetric Presentation State Input Sequence (0070,1201) and generates an RGB and an Alpha output. This classification component would be specified in an item of the Presentation State Classification Component Sequence (0070,1801):

  Figure FF.2-3. One Input -> RGBA Component

- Two Inputs -> RGBA: This component accepts reconstructed data from two inputs in the Volumetric Presentation State Input Sequence (0070,1201) and generates an RGB and an Alpha output. This component is used in the case where a two-dimensional color mapping needs to be performed. This classification component would be specified in an item of the Presentation State Classification Component Sequence (0070,1801):

  Figure FF.2-4. Two Inputs ->RGBA Component

  ### Note

  An example for the use of this component is to combine Ultrasound Flow Velocity and Ultrasound Flow Variance to produce a color range from red-blue based on flow velocity and adding a yellow-green tinge based on flow variance)

Prev | Up | Next
FF.2.3 Volumetric Presentation State Display | Home | FF.2.3.2.2 Compositor Components

DICOM PS3.4 2020d - Service Class Specifications