DICOM PS3.3 2020d - Information Object Definitions

A.34.12 Routine Scalp Electroencephalogram IOD (Current)
Prev | A.34 Waveform Information Object Definitions | Next

### A.34.12 Routine Scalp Electroencephalogram IOD

#### A.34.12.1 Routine Scalp Electroencephalogram IOD Description

The Routine Scalp Electroencephalogram (EEG) IOD is the specification of digitized electrical signals from the patient's encephalon collected on the skull surface, which has been acquired by an EEG modality or by an EEG acquisition function within an imaging modality or a neurophysiology recording device.

### Note

This type of object could cover these clinical scenarios:

- Routine EEG

- EEG-Video-Monitoring - scalp EEG

as these have similar physical properties and use the same electrode location scheme.

Prev | Up | Next
A.34.11.4.8 Time Distribution Protocol | Home | A.34.12.2 Routine Scalp Electroencephalogram IOD Entity-Relationship Model

DICOM PS3.3 2020d - Information Object Definitions