DICOM PS3.2 2020d - Conformance

B.4.3.2 Additional Protocols (Current)
Prev | B.4.3 Network Interfaces | Next

#### B.4.3.2 Additional Protocols

EXAMPLE-INTEGRATED-MODLALITY conforms to the System Management Profiles listed in the Table below. All requested transactions for the listed profiles and actors are supported. Support for optional transactions are listed in the Table below:

Table B.4.3-2. Supported System Management Profiles

Profile Name | Actor | Protocols Used | Optional Transactions | Security Support
--- | --- | --- | --- | ---
Network Address Management | DHCP Client | DHCP | N/A |
DNS Client | DNS | N/A |
Time Synchronization | NTP Client | NTP | Find NTP Server |
DHCP Client | DHCP | N/A |
DICOM Application Configuration Management | LDAP Client | LDAP | Client Update LDAP Server | See Section B.7

##### B.4.3.2.1 DHCP

DHCP can be used to obtain TCP/IP network configuration information. The network parameters obtainable via DHCP are shown in the Table below. The Default Value column of the table shows the default used if the DHCP server does not provide a value. Values for network parameters set in the Service/Installation tool take precedence over values obtained from the DHCP server. Support for DHCP can be configured via the Service/Installation Tool. The Service/Installation tool can be used to configure the machine name. If DHCP is not in use, TCP/IP network configuration information can be manually configured via the Service/Installation Tool.

Table B.4.3-3. Supported DHCP Parameters

DHCP Parameter | Default Value
IP Address | None
Hostname | Requested machine name
List of NTP servers | Empty list
List of DNS servers | Empty list
Routers | Empty list
Static routes | None
Domain name | None
Subnet mask | Derived from IP Address (see service manual)
Broadcast address | Derived from IP Address (see service manual)
Default router | None
Time offset | Site configurable (from Timezone)
MTU | Network Hardware Dependent
Auto-IP permission | No permission

If the DHCP server refuses to renew a lease on the assigned IP address all active DICOM Associations will be aborted.

Prev | Up | Next
B.4.3 Network Interfaces | Home | B.4.3.2.2 DNS

DICOM PS3.2 2020d - Conformance