DICOM PS3.11 2020d - Media Storage Application Profiles

K.3.4.2 Image Attribute Specialization (Current)
Prev | K.3.4 Other Parameters | Next

#### K.3.4.2 Image Attribute Specialization

The Attributes listed in Table K.3-4 shall have their Types specialized.

Table K.3-4. STD-DEN-CD - Required Image Attribute Types

Attribute | Tag | Type
--- | --- | ---
Institution Name | (0008,0080) | 2
Manufacturer's Model Name | (0008,1090) | 2
Detector ID | (0018,700A) | 2
Detector Manufacturer Name | (0018,702A) | 2
Detector Manufacturer's Model Name | (0018,702B) | 2

### Note

These Type 3 attributes of the General Equipment and DX Detector Module are specialized in order to encourage FSCs to include values for them, recognizing that there are situations in which values may be unknown.

Prev | Up | Next
K.3.4 Other Parameters | Home | L ZIP File Over Email Interchange Profiles (Normative)

DICOM PS3.11 2020d - Media Storage Application Profiles