DICOM PS3.3 2020d - Information Object Definitions

A.83.3 Ophthalmic Optical Coherence Tomography En Face Image IOD Modules (Current)
Prev | A.83 Ophthalmic Optical Coherence Tomography En Face Image IOD | Next

### A.83.3 Ophthalmic Optical Coherence Tomography En Face Image IOD Modules

Table A.83-1 specifies the Modules of the Ophthalmic Optical Coherence Tomography En Face Image IOD.

Table A.83-1. Ophthalmic Optical Coherence Tomography En Face Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Ophthalmic Tomography En Face Series | C.8.17.17 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | M
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | General Image | C.7.6.1 | M
Image Pixel | C.7.6.3 | M
Palette Color Lookup Table | C.7.9 | C - Required if Photometric Interpretation (0028,0004) has a value of PALETTE COLOR
Ophthalmic Optical Coherence Tomography En Face Image | C.8.17.14 | M
Ocular Region Imaged | C.8.17.5 | M
Ophthalmic Optical Coherence Tomography En Face Image Quality Rating | C.8.17.15 | C - Required if device calculates quality rating
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U

Prev | Up | Next
A.83.2 Ophthalmic Optical Coherence Tomography En Face Image IOD Entity-Relationship Model | Home | A.83.4 Ophthalmic Optical Coherence Tomography En Face Image IOD Content Constraints

DICOM PS3.3 2020d - Information Object Definitions