DICOM PS3.3 2020d - Information Object Definitions

A.8.5.2 Multi-frame True Color SC Image IOD Entity-Relationship Model (Current)
Prev | A.8.5 Multi-frame True Color Secondary Capture Image IOD | Next

#### A.8.5.2 Multi-frame True Color SC Image IOD Entity-Relationship Model

This IOD uses the E-R Model in Section A.1.2, with only the Image IE below the Series IE.

Prev | Up | Next
A.8.5 Multi-frame True Color Secondary Capture Image IOD | Home | A.8.5.3 Multi-frame True Color SC Image IOD Module Table

DICOM PS3.3 2020d - Information Object Definitions