DICOM PS3.3 2020e - Information Object Definitions

C.11.27.4 Weighting Transfer Function (Current)
Prev | C.11.27 MPR Volumetric Presentation State Display Module | Next

#### C.11.27.4 Weighting Transfer Function

In some situations, it is desirable to consider both Alpha inputs to the compositor in determining the weight to be given to each of the two RGB inputs to the compositing operation. This is accomplished by providing two weighting transfer functions

f(Alpha1,Alpha2) = WeightingFactorn

one for each of the two RGB inputs to the compositor.

In the degenerate (and common) case where simple additive compositing (RGB1*Alpha1)+(RGB2* (1-Alpha1)) is desired, identity weighting transfer functions can be specified to just pass through the Alpha 1and (1-Alpha 1) values (or Alpha 1and Alpha 2values) to be the weighing factors for the RGB inputs.

For ease of specification of these transfer functions and for maximum flexibility, each of these weighting transfer functions is defined as a look-up table with inputs Alpha1 and Alpha2. Each LUT contains 8-bit integer values which are then normalized to the range 0.0 to 1.0 by dividing by 255 (28-1).

See Section FF.2.3.3.2 “Internal Structure of RGB and RGBA Compositor Components” in PS3.4 for details on the use of these weighting transfer functions, and see Section XXX.5 “Compositing and the Use of Weighting Transfer Functions” in PS3.17 for clinical applications.

Prev | Up | Next
C.11.27.3 Compositor Component Usage | Home | C.11.27.5 Use of Segmented Palette Color Lookup Tables

DICOM PS3.3 2020e - Information Object Definitions