DICOM PS3.4 2020e - Service Class Specifications

H.4.9.2.2 N-DELETE (Current)
Prev | H.4.9.2 DIMSE Service Group | Next

##### H.4.9.2.2 N-DELETE

The N-DELETE Service Element is used to delete the Presentation LUT SOP Instance.

###### H.4.9.2.2.1 Status

There are no specific status codes. See PS3.7 for response status codes.

###### H.4.9.2.2.2 Behavior

The SCU uses the N-DELETE Service Element to request the SCP to delete the Presentation LUT SOP Instance. The SCU shall specify the Presentation LUT SOP Instance UID.

The SCP shall not delete a Presentation LUT SOP Instance as long as there are outstanding references to it. Otherwise, it shall delete the specified Presentation LUT SOP Instance. The N-DELETE of a Presentation LUT will prevent the SCU from further referencing it. The SCU shall not reference a previously deleted Presentation LUT. The SCP shall return the status code of the requested Presentation LUT SOP Instance deletion. The meaning of success, warning, and failure status codes is defined in Section H.2.5.

Prev | Up | Next
H.4.9.2 DIMSE Service Group | Home | H.4.9.2.4 SOP Class Definition and UID

DICOM PS3.4 2020e - Service Class Specifications