DICOM PS3.3 2020e - Information Object Definitions

A.32.7.3 Video Photographic Image IOD Module Table (Current)
Prev | A.32.7 Video Photographic Image IOD | Next

#### A.32.7.3 Video Photographic Image IOD Module Table

Table A.32.7-1 specifies the Modules of the Video Photographic Image IOD.

Table A.32.7-1. Video Photographic Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Synchronization | C.7.4.2 | U
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Cine | C.7.6.5 | M
Multi-frame | C.7.6.6 | M
Image Pixel | C.7.6.3 | M
Acquisition Context | C.7.6.14 | M
Device | C.7.6.12 | U
Specimen | C.7.6.22 | C - Required if the Imaging Subject is a Specimen
VL Image | C.8.12.1 | M
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

Prev | Up | Next
A.32.7.2 Video Photographic Image IOD Entity-Relationship Model | Home | A.32.7.4 Video Photographic Image IOD Content Constraints

DICOM PS3.3 2020e - Information Object Definitions