DICOM PS3.4 2020e - Service Class Specifications

DD.3.2.5 N-EVENT-REPORT (Current)
Prev | DD.3.2 DIMSE Service Group | Next

#### DD.3.2.5 N-EVENT-REPORT

The N-EVENT-REPORT is used by the MPV to notify the TDS of the status of the verification task (successful or otherwise), or to notify the TDS that a verification is pending (in progress). The encoding of Notification Event Information is defined in PS3.7.

##### DD.3.2.5.1 Attributes

The arguments of the N-EVENT-REPORT are defined as shown in Table DD.3.2.5-1.

Table DD.3.2.5-1. Notification Event Information

Event Type Name | Event Type ID | Attribute Name | Tag | Usage SCU/SCP
--- | --- | --- | --- | ---
Pending | 1 | None | - | -
Done | 2 | Treatment Verification Status | (3008,002C) | -/1

Prev | Up | Next
DD.3.2.4.3 Behavior | Home | DD.3.2.5.2 Status

DICOM PS3.4 2020e - Service Class Specifications