DICOM PS3.3 2020e - Information Object Definitions

C.8.8.29.3 Meterset Exposure (Current)
Prev | C.8.8.29 RT Beams Delivery Instruction Module | Next

##### C.8.8.29.3 Meterset Exposure

Meterset Exposure (3002,0032) can be interpreted as the 'maximum' Meterset duration in cases where an automatic exposure is taken.

Prev | Up | Next
C.8.8.29.2 Adjusted Table Positions and Angles | Home | C.8.8.29.4 Double Exposure Field Delta

DICOM PS3.3 2020e - Information Object Definitions