DICOM PS3.3 2020e - Information Object Definitions

C.8.21.3.3 X-Ray 3D Craniofacial Acquisition Module (Current)
Prev | C.8.21.3 X-Ray 3D Acquisition Modules | Next

##### C.8.21.3.3 X-Ray 3D Craniofacial Acquisition Module

This section describes the X-Ray 3D Craniofacial Acquisition Module.

Table C.8.21.3.3-1. X-Ray 3D Craniofacial Acquisition Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
X-Ray 3D Acquisition Sequence | (0018,9507) | 1 | Each Item represents a acquisition context related to a set of frames of SOP Instance defined by this IOD, The values of Acquisition Index (0020,9518) may be used as index to Items in this Sequence. One or more Items shall be included in this Sequence.
>Field of View Shape | (0018,1147) | 1C | Shape of the Field of View in the referenced images. Enumerated Values: RECTANGLE ROUND HEXAGONAL Required if present and consistent in the contributing SOP Instances.
>X-Ray Receptor Type | (0018,9420) | 1C | Identifies the type of X-Ray receptor used. Enumerated Values: DIGITAL_DETECTOR Required if present and consistent in the contributing SOP Instances.
>Include Table C.8.21.3.1.1-1 “X-Ray 3D General Shared Acquisition Macro Attributes” |
>Include Table C.8-71b “Digital X-Ray Detector Macro Attributes” |
>Per Projection Acquisition Sequence | (0018,9538) | 1C | Sequence containing detailed acquisition context of each individual projection used in this acquisition context. One or more Items shall be included in this Sequence. Required if present and consistent in the contributing SOP Instances.
>>Include Table C.8.21.3.1.2-1 “X-Ray 3D General Per Projection Acquisition Macro Attributes” |

Prev | Up | Next
C.8.21.3.2 X-Ray 3D Angiographic Acquisition Module | Home | C.8.21.3.4 Breast Tomosynthesis Acquisition Module

DICOM PS3.3 2020e - Information Object Definitions