DICOM PS3.4 2020e - Service Class Specifications

H.2.5 Status Code Categories (Current)
Prev | H.2 Print Management Model | Next

### H.2.5 Status Code Categories

For every operation requested on a SOP Class of the print management service class, a status code will be returned. These status codes are grouped into success, warning or failure categories.

### Note

These status codes categories are defined in PS3.7:

- Success - indicates that the SCP performed the requested operation as requested.

- Warning - indicates that the SCP has received the request and will process it. However, immediate processing of the request, or processing in the way specified by the SCU, may not be possible. The SCP expects to be able to complete the request without further action by the SCU across the DICOM interface. The exact behavior of the SCP is described in the Conformance Statement.

- Failure - indicates that the SCP is unable to perform the request. The request will not be processed unless it is repeated by the SCU at a later time. The exact behavior of the SCP is described in the Conformance Statement.

Prev | Up | Next
H.2.4 Usage Specifications | Home | H.3 Print Management Conformance

DICOM PS3.4 2020e - Service Class Specifications