DICOM PS3.17 2020e - Explanatory Information

S.6.4 Association Requesters On Legacy Nodes (Current)
Prev | S.6 Switching A Node From Unmanaged to Managed in A Mixed Network | Next

### S.6.4 Association Requesters On Legacy Nodes

These will probably remain unchanged. The IP address must be pre-allocated if there are legacy nodes that cannot support DHCP.

Prev | Up | Next
S.6.3 Association Acceptors On This Node | Home | S.6.5 Association Requesters On Managed Nodes

DICOM PS3.17 2020e - Explanatory Information