DICOM PS3.3 2020e - Information Object Definitions

A.32.10.3 Real-Time Video Photographic Image IOD Module Table (Current)
Prev | A.32.10 Real-Time Video Photographic Image IOD | Next

#### A.32.10.3 Real-Time Video Photographic Image IOD Module Table

Table A.32.10-1 specifies the Modules of the Real-Time Video Photographic Image IOD.

Table A.32.10-1. Real-Time Video Photographic Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Frame of Reference | Frame of Reference | C.7.4.1 | C - Required if multiple Instances are spatially related or if the Camera Position Functional Group Module is present in the Current Frame Functional Groups Module
Synchronization | C.7.4.2 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Real-Time Bulk Data Flow | C.7.6.26 | M
Acquisition Context | C.7.6.14 | M
Device | C.7.6.12 | U
Specimen | C.7.6.22 | C - Required if the Imaging Subject is a Specimen
VL Image | C.8.12.1 | M
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | M
Real-Time Acquisition | C.7.6.28 | M
Current Frame Functional Groups | C.7.6.27 | M

Prev | Up | Next
A.32.10.2 Real-Time Video Photographic Image IOD Entity-Relationship Model | Home | A.32.10.4 Real-Time Video Photographic Image IOD Content Constraints

DICOM PS3.3 2020e - Information Object Definitions