DICOM PS3.16 2020e - Content Mapping Resource

TID 4014 CAD Image Quality (Current)
Prev | Mammography CAD SR IOD Templates | Next

### TID 4014 CAD Image Quality

This Template provides the detail specific to image quality. It allows the encoding of descriptors of image quality (e.g., CID 6041 “Mammography Image Quality Finding”) for a given image or region of an image. For instance, images with partial motion blur can be identified with the region noted.

Table TID 4014. Parameters

Parameter Name | Parameter Usage
--- | ---
$QualityFinding | Coded term or Context Group for Quality Finding
$QualityStandard | Coded term or Context Group for Quality Control Standard

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4014. CAD Image Quality

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (111052, DCM, "Quality Finding") | 1 | M |  | $QualityFinding
2 | > | HAS PROPERTIES | CODE | EV (111050, DCM, "Quality Assessment") | 1 | U |  | DCID 6044 “Types of Image Quality Assessment”
3 | > | HAS PROPERTIES | CODE | EV (111051, DCM, "Quality Control Standard") | 1 | UC | Shall be present if row 2 is present. | $QualityStandard
4 | > | HAS PROPERTIES | NUM | EV (111029, DCM, "Image Quality Rating") | 1 | U |  | UNITS = EV (%, UCUM, "Percent") Value = 0 - 100

Content Item Descriptions

Image Quality Rating | A numeric value in the range 0 to 100, inclusive, where 0 is worst quality and 100 is best quality.

Prev | Up | Next
TID 4013 Mammography CAD Selected Region | Home | TID 4015 CAD Detections Performed

DICOM PS3.16 2020e - Content Mapping Resource