DICOM PS3.4 2020e - Service Class Specifications

EE.2 Display System SOP Class (Current)
Prev | EE Display System Management Service Class (Normative) | Next

## EE.2 Display System SOP Class

### EE.2.1 IOD Description

The Display System IOD is an abstraction of the soft-copy display system and is the basic Information Entity to monitor the status of a Display System. The Display System SOP Instance is created by the SCP during start-up of the Display System and has a well-known SOP Instance UID.

Prev | Up | Next
EE Display System Management Service Class (Normative) | Home | EE.2.2 DIMSE Service Group

DICOM PS3.4 2020e - Service Class Specifications