DICOM PS3.17 2020e - Explanatory Information

XXX.3.4.3 Encoding Details (Current)
Prev | XXX.3.4 Replacing Set of Derived Images With Single VPS Using Crosscurve Animation | Next

#### XXX.3.4.3 Encoding Details

##### XXX.3.4.3.1 Presentation Animation Module Recommendations

Table XXX.3.4-1. Presentation Animation Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Presentation Animation Style | (0070,1A01) | Set to "CROSSCURVE"
Recommended Animation Rate | (0070,1A03) | Set to provide a hint to the display application to automatically move the Planar MPR view along the curve through the volume, or omitted to leave the animation method to the discretion of the display application.
Animation Curve Sequence | (0070,1A04) | Set to the start point and end point of the straight-line curve.
Animation Step Size | (0070,1A05) | Set to (line length / (number of slices - 1)) as the distance between MPR views along the straight-line curve.

Prev | Up | Next
XXX.3.4.2 Encoding Outline | Home | XXX.3.5 Volumetric Annotations (example: Trajectory Planning)

DICOM PS3.17 2020e - Explanatory Information