DICOM PS3.15 2021b - Security and System Management Profiles

B.5 User Identity Plus Passcode Association Profile (Current)
Prev | B Secure Transport Connection Profiles (Normative) | Next

## B.5 User Identity Plus Passcode Association Profile

An implementation that supports the User Identity plus Passcode Association Profile shall send/accept the User Identity association negotiation sub-item, for User-Identity-Type of 2. If a positive response is requested, the association acceptor implementation shall respond with the association response sub-item. The passcode information shall be made available to internal or external authentication systems. The user identity shall be authenticated by means of the passcode and the authentication system. If the authentication fails, the association shall be rejected.

The user identity from the Primary-field shall be used within the implementation as the user identification. Such uses include recording user identification in audit messages.

Table B.5-1. User Identity Plus Passcode Association Profile - Minimum Mechanisms for DICOM Association Negotiation Features

Supported Association Negotiation Feature | Minimum Mechanism
--- | ---
User Identity | Username and Passcode

Prev | Up | Next
B.4 Basic User Identity Association Profile | Home | B.6 Kerberos Identity Negotiation Association Profile

DICOM PS3.15 2021b - Security and System Management Profiles