DICOM PS3.16 2021b - Content Mapping Resource

TID 10045 Radiation Technique (Current)
Prev | Enhanced X-Ray Radiation Dose SR IOD Templates | Next

### TID 10045 Radiation Technique

This template describes the technique parameters (e.g., X-Ray tube potential, X-Ray tube current, pulse rate, etc.) of the radiation exposure during a period of time.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10045. Radiation Technique

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (130511, DCM, "Radiation Technique") | 1 | M |  |
2 | > | CONTAINS | DATETIME | DT (111526, DCM, "DateTime Started") | 1 | M |  |
3 | > | CONTAINS | DATETIME | DT (111527, DCM, "DateTime Ended") | 1 | M |  |
4 | > | CONTAINS | TEXT | EV (113832, DCM, "Identification of the X-Ray Source") | 1 | M |  |
5 | > | CONTAINS | NUM | EV (111634, DCM, "Half Value Layer") | 1 | UC | XOR Row 7 | UNITS = EV (mm, UCUM, "mm")
6 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
7 | > | CONTAINS | TABLE | EV (111634, DCM, "Half Value Layer") | 1 | UC | XOR Row 5 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (111634, DCM, "Half Value Layer") COLUMN 2 UNITS = EV (mm, UCUM, "mm") COLUMN 1 VR = DT COLUMN 2 VR = FL
8 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
9 | > | CONTAINS | NUM | EV (113733, DCM, "KVP") | 1 | MC | XOR Row 11 | UNITS = EV (kV, UCUM, "kV")
10 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
11 | > | CONTAINS | TABLE | EV (113733, DCM, "KVP") | 1 | MC | XOR Row 9 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113733, DCM, "KVP") COLUMN 2 UNITS = EV (kV, UCUM, "kV") COLUMN 1 VR = DT COLUMN 2 VR = FL
12 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
13 | > | CONTAINS | NUM | EV (113734, DCM, "X-Ray Tube Current") | 1 | MC | XOR Row 15 | UNITS = EV (mA, UCUM, "mA")
14 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
15 | > | CONTAINS | TABLE | EV (113734, DCM, "X-Ray Tube Current") | 1 | MC | XOR Row 13 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113734, DCM, "X-Ray Tube Current") COLUMN 2 UNITS = EV (mA, UCUM, "mA") COLUMN 1 VR = DT COLUMN 2 VR = FL
16 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
17 | > | CONTAINS | NUM | EV (113791, DCM, "Pulse Rate") | 1 | UC | XOR Row 19 | UNITS = EV ({pulse}/s, UCUM, "pulse/s")
18 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
19 | > | CONTAINS | TABLE | EV (113791, DCM, "Pulse Rate") | 1 | UC | XOR Row 17 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113791, DCM, "Pulse Rate") COLUMN 2 UNITS = EV ({pulse}/s, UCUM, "pulse/s") COLUMN 1 VR = DT COLUMN 2 VR = FL
20 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
21 | > | CONTAINS | NUM | EV (113793, DCM, "Pulse Width") | 1 | UC | XOR Row 23 | UNITS = EV (ms, UCUM, "ms")
22 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”
23 | > | CONTAINS | TABLE | EV (113793, DCM, "Pulse Width") | 1 | UC | XOR Row 21 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113793, DCM, "Pulse Width") COLUMN 2 UNITS = EV (ms, UCUM, "ms") COLUMN 1 VR = DT COLUMN 2 VR = FL
24 | >> | HAS PROPERTIES | CODE | EV (130510, DCM, "Reported Value Type") | 1 | U |  | DCID 10072 “Reported Value Types”

Content Item Descriptions

Row 2 | The DateTime of the beginning of the time period over which the content items are applicable.
Row 3 | The DateTime of the end of the time period over which the content items are applicable.
Row 4 | Identification the X-Ray source. This designation shall not change for a given source throughout the entire RDSR. For systems with multiple X-Ray sources, each source shall be described with a separate instance of this template.

Prev | Up | Next
TID 10044 Radiation Source Characteristics | Home | TID 10046 Filtration

DICOM PS3.16 2021b - Content Mapping Resource