DICOM PS3.3 2021b - Information Object Definitions

A.34.16.4.3 Sampling Frequency (Current)
Prev | A.34.16.4 Multi-channel Respiratory Waveform IOD Constraints | Next

##### A.34.16.4.3 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence Item is not constrained.

Prev | Up | Next
A.34.16.4.2 Waveform Sequence and Number of Waveform Channels | Home | A.34.16.4.4 Channel Source and Channel Source Modifiers

DICOM PS3.3 2021b - Information Object Definitions