DICOM PS3.16 2021b - Content Mapping Resource

Enhanced X-Ray Radiation Dose SR IOD Templates (Current)
Prev | A Structured Reporting Templates (Normative) | Next

## Enhanced X-Ray Radiation Dose SR IOD Templates

The Templates that comprise the Enhanced X-Ray Radiation Dose SR are interconnected as in Figure A-18b.

Figure A-18b. Enhanced X-Ray Radiation Dose Structured Report IOD Template Structure

### TID 10040 Enhanced X-Ray Radiation Dose

This template defines a container (the root) with subsidiary content items for documenting the radiation output for an ionizing radiation imaging device. This template supports cone-beam CT, in addition to other modalities.

Type:

  Extensible

Order:

  Non-Significant

Root:

  Yes

Table TID 10040. Enhanced X-Ray Radiation Dose

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (113701, DCM, "X-Ray Radiation Dose Report") | 1 | M |  | Root Node
2 | > | HAS CONCEPT MOD | INCLUDE | DTID 1204 “Language of Content Item and Descendants” | 1 | M |  |
3 | > | HAS CONCEPT MOD | CODE | EV (121058, DCM, "Procedure reported") | 1 | M |  |
4 | >> | HAS CONCEPT MOD | CODE | EV (363703001, SCT, "Has Intent") | 1 | M |  | DCID 3629 “Procedure Intent”
5 | > | HAS OBS CONTEXT | INCLUDE | DTID 1002 “Observer Context” | 1-n | M |  |
6 | > | HAS OBS CONTEXT | CODE | EV (113705, DCM, "Scope of Accumulation") | 1 | M |  | DCID 10000 “Scope of Accumulation”
7 | > | CONTAINS | INCLUDE | DTID 10041 “Accumulated Dose Data” | 1-n | U |  |
8 | > | CONTAINS | INCLUDE | DTID 10042 “Irradiation Event Summary Data” | 1-n | M |  |
9 | > | CONTAINS | INCLUDE | DTID 10043 “Irradiation Details” | 1 | M |  |
10 | > | CONTAINS | TEXT | EV (121106, DCM, "Comment") | 1 | U |  |
11 | > | CONTAINS | INCLUDE | DTID 1020 “Person Participant” | 1 | U |  | $PersonProcedureRole = EV (113850, DCM, "Irradiation Authorizing")
12 | > | CONTAINS | CODE | EV (113854, DCM, "Source of Dose Information") | 1-n | M |  | DCID 10020 “Source of Projection X-Ray Dose Information”

Content Item Descriptions

Row 7 | TID 10041 may be included once for each source. Summary-level values that may include multiple sources, e.g., Dose Area Product Total from planes A and B of a biplane system,could be described by an instance of TID 10041 where the Identification of X-Ray Source indicates multiple sources, e.g., "A and B".
Row 8 | TID 10042 shall be included once for each irradiation event. Irradiation event values that may include multiple sources, e.g., CTDI for a dual-source CT scanner,could be described by an instance of TID 10042 where the Identification of X-Ray Source indicates multiple sources, e.g., "1 and 2".

Prev | Up | Next
TID 10034 Radiation Dose Estimate Parameters | Home | TID 10041 Accumulated Dose Data

DICOM PS3.16 2021b - Content Mapping Resource