DICOM PS3.2 2021b - Conformance

H.4.4.2 Parameters (Current)
Prev | H.4.4 Configuration | Next

#### H.4.4.2 Parameters

Table H.4.4-2. Configuration Parameters

Parameter | Configurable | Default Value
--- | --- | ---
General Parameters
Maximum PDU size I can receive | Yes | 128kbytes
Maximum PDU size I can send | Yes | 128kbytes
Time-out waiting for response to TCP/IP connect() request. (Low-level timeout) | Yes | 10 s
Time-out waiting for A-ASSOCIATE RQ PDU on open TCP/IP connection. (ARTIM timeout) | Yes | 30 s
Time-out waiting for acceptance or rejection response to an Association Open Request. (Application Level timeout) | Yes | 30s
Time-out waiting for acceptance of a TCP/IP message over the network. (Low-level timeout) | Yes | 30 s
Time-out for waiting for data between TCP/IP packets. (Low-level timeout) | Yes | 30 s
PHARMACY-SCP AE Parameters
Maximum number of simultaneous Associations | Yes | 10
AE time-out waiting on an open Association for the next message (C-FIND-RQ, Association Close Request. etc.) (DIMSE timeout) | Yes | 1 minute
MAR-SCP AE Parameters
Maximum number of simultaneous Associations | Yes | 10
AE time-out waiting on an open Association for the next Request message (N-ACTION-RQ, Association Close Request. etc.) (DIMSE timeout) | Yes | 1 minute

Prev | Up | Next
H.4.4 Configuration | Home | H.5 Media Interchange

DICOM PS3.2 2021b - Conformance