DICOM PS3.2 2021b - Conformance

L.4 Networking (Current)
Prev | L Conformance Statement Sample DICOM-RTV Service Provider (Informative) | Next

## L.4 Networking

### L.4.1 Implementation Model

#### L.4.1.1 Application Data Flow

Figure L.4.1-1. Application Data Flow Diagram

The DICOM-RTV Service Application provides multiple DICOM-RTV compliant Flows, transported in RTP over IP, that can be consumed by one or multiple other DICOM-RTV Service Application(s).

#### L.4.1.2 Functional Definition of AEs

##### L.4.1.2.1 Functional Definition of RTV Service Application

The DICOM-RTV Service is Active when the equipment produces video content.

Prev | Up | Next
L.3.3 Additional Remarks for This Example | Home | L.4.2 AE Specifications

DICOM PS3.2 2021b - Conformance