DICOM PS3.15 2021b - Security and System Management Profiles

A.5.3.10 Query (Current)
Prev | A.5.3 DICOM Specific Audit Messages | Next

#### A.5.3.10 Query

This message describes the event of a Query being issued or received. The message does not record the response to the query, but merely records the fact that a query was issued. For example, this would report queries using the DICOM SOP Classes:

1. Modality Worklist

2. UPS Pull

3. UPS Watch

4. Composite Instance Query

### Note

1. The response to a query may result in one or more Instances Transferred or Instances Accessed messages, depending on what events transpire after the query. If there were security-related failures, such as access violations, when processing a query, those failures should show up in other audit messages, such as a Security Alert message.

2. Non-DICOM queries may also be captured by this message. The Participant Object ID Type Code, the Participant Object ID, and the Query fields may have values related to such non-DICOM queries.

Table A.5.3.10-1. Audit Message for Query

Real World Entities | Field Name | Opt. | Value Constraints
--- | --- | --- | ---
Event | EventID | M | EV (110112, DCM, "Query")
EventActionCode | M | Shall be: E = Execute
EventDateTime | M | not specialized
EventOutcomeIndicator | M | not specialized
EventTypeCode | U | not specialized
Active Participant: Process Issuing the Query (1) | UserID | M | not specialized
AlternativeUserID | U | not specialized
UserName | U | not specialized
UserIsRequestor | M | not specialized
RoleIDCode | M | EV (110153, DCM, "Source Role ID")
NetworkAccessPointTypeCode | U | not specialized
NetworkAccessPointID | U | not specialized
Active Participant: The process that will respond to the query (1) | UserID | M | not specialized
AlternativeUserID | U | not specialized
UserName | U | not specialized
UserIsRequestor | M | not specialized
RoleIDCode | M | EV (110152, DCM, "Destination Role ID")
NetworkAccessPointTypeCode | U | not specialized
NetworkAccessPointID | U | not specialized
Active Participant: Other Participants that are known, especially third parties that requested the query (0..N) | UserID | M | not specialized
AlternativeUserID | U | not specialized
UserName | U | not specialized
UserIsRequestor | M | not specialized
RoleIDCode | U | not specialized
NetworkAccessPointTypeCode | U | not specialized
NetworkAccessPointID | U | not specialized
Participating Object: SOP Queried and the Query (1) | ParticipantObjectTypeCode | M | Shall be: 2 = system
ParticipantObjectTypeCodeRole | M | Shall be: 3 = report
ParticipantObjectDataLifeCycle | U | not specialized
ParticipantObjectIDTypeCode | M | DT (110181, DCM, "SOP Class UID")
ParticipantObjectSensitivity | U | not specialized
ParticipantObjectID | M | If the ParticipantObjectIDTypeCode is (110181, DCM, "SOP Class UID"), then this field shall hold the UID of the SOP Class being queried
ParticipantObjectName | U | not specialized
ParticipantObjectQuery | M | If the ParticipantObjectIDTypeCode is (110181, DCM, "SOP Class UID"), then this field shall hold the Dataset of the DICOM query, xs:base64Binary encoded. Otherwise, it shall be the query in the format of the protocol used.
ParticipantObjectDetail | MC | Required if the ParticipantObjectIDTypeCode is (110181, DCM, "SOP Class UID") A ParticipantObjectDetail element with the XML attribute "TransferSyntax" shall be present. The value of the Transfer Syntax attribute shall be the UID of the transfer syntax of the query. The element contents shall be xs:base64Binary encoding. The Transfer Syntax shall be a DICOM Transfer Syntax.
ParticipantObjectDescription | U | not specialized
SOPClass | U | See Table A.5.2-1
Accession | U | not specialized
NumberOfInstances | U | not specialized
Instances | U | not specialized
Encrypted | U | not specialized
Anonymized | U | not specialized

Prev | Up | Next
A.5.3.9 Network Entry | Home | A.5.3.11 Security Alert

DICOM PS3.15 2021b - Security and System Management Profiles