DICOM PS3.3 2021b - Information Object Definitions

A.82.5.3 XA Defined Procedure Protocol IOD Module Table (Current)
Prev | A.82.5 XA Defined Procedure Protocol IOD | Next

#### A.82.5.3 XA Defined Procedure Protocol IOD Module Table

Table A.82.5.3-1. XA Defined Procedure Protocol IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Procedure Protocol | Protocol Context | C.34.2 | M
Clinical Trial Context | C.34.4 | U
Patient Specification | C.34.5 | U
Equipment Specification | C.34.6 | M
Instructions | C.34.7 | U
Patient Positioning | C.34.8 | U
General Defined Acquisition | C.34.9 | U
General Defined Reconstruction | C.34.11 | U
Defined Storage | C.34.13 | U
SOP Common | C.12.1 | M

##### A.82.5.3.1 XA Defined Procedure Protocol IOD Content Constraints

###### A.82.5.3.1.1 Equipment Modality Attribute

The value of Equipment Modality (0008,0221) shall be XA.

### Note

An application can query for Protocols by matching on the modality-specific Defined Protocol SOP Class.

Prev | Up | Next
A.82.5.2 XA Defined Procedure Protocol IOD Entity-Relationship Model | Home | A.83 Ophthalmic Optical Coherence Tomography En Face Image IOD

DICOM PS3.3 2021b - Information Object Definitions