DICOM PS3.16 2021b - Content Mapping Resource

TID 10041 Accumulated Dose Data (Current)
Prev | Enhanced X-Ray Radiation Dose SR IOD Templates | Next

### TID 10041 Accumulated Dose Data

This template documents scope of accumulation summary data for a single radiation source. Some rows are modality-specific and may not apply to all uses.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10041. Accumulated Dose Data

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (130500, DCM, "Accumulated Dose Data") | 1 | M |  |
2 | > | CONTAINS | TEXT | EV (113832, DCM, "Identification of the X-Ray Source") | 1 | M |  |
3 | > | CONTAINS | CONTAINER | EV (122505, DCM, "Calibration") | 1-n | MC | IFF Calibration Data is available |
4 | >> | HAS CONCEPT MOD | CODE | EV (113794, DCM, "Dose Measurement Device") | 1 | M |  | DCID 10010 “Dose Measurement Devices” DCID 7026 “Radiotherapeutic Dose Measurement Devices”
5 | >> | CONTAINS | DATETIME | EV (113723, DCM, "Calibration DateTime") | 1 | M |  |
6 | >> | CONTAINS | NUM | EV (122322, DCM, "Calibration Factor") | 1 | M |  | UNITS = EV (1, UCUM, "no units")
7 | >> | CONTAINS | NUM | EV (113763, DCM, "Calibration Uncertainty") | 1 | M |  | UNITS = EV (%, UCUM, "Percent")
8 | >> | CONTAINS | TEXT | EV (113724, DCM, "Calibration Responsible Party") | 1 | M |  |
9 | >> | CONTAINS | TEXT | EV (113720, DCM, "Calibration Protocol") | 1 | U |  |
10 | > | CONTAINS | INCLUDE | DTID 1021 “Device Participant” | 1 | MC | Required if the irradiating device is not the recording device and the dose was accumulated on a single device. | $DeviceProcedureRole = EV (113859, DCM, "Irradiating Device")
11 | > | CONTAINS | NUM | EV (113722, DCM, "Dose Area Product Total") | 1 | U |  | UNITS = EV (Gy.m2, UCUM, "Gy.m2")
12 | > | CONTAINS | NUM | EV (113726, DCM, "Fluoro Dose Area Product Total") | 1 | U |  | UNITS = EV (Gy.m2, UCUM, "Gy.m2")
13 | > | CONTAINS | NUM | EV (113727, DCM, "Acquisition Dose Area Product Total") | 1 | U |  | UNITS = EV (Gy.m2, UCUM, "Gy.m2")
14 | > | CONTAINS | NUM | EV (113730, DCM, "Total Fluoro Time") | 1 | U |  | UNITS = EV (s, UCUM, "s")
15 | > | CONTAINS | NUM | EV (113855, DCM, "Total Acquisition Time") | 1 | U |  | UNITS = EV (s, UCUM, "s")
16 | > | CONTAINS | NUM | EV (111637, DCM, "Accumulated Average Glandular Dose") | 1-2 | U |  | UNITS = EV (mGy, UCUM, "mGy")
17 | >> | HAS CONCEPT MOD | CODE | EV (272741003, SCT, "Laterality") | 1 | M |  | DCID 6022 “Side”
18 | > | CONTAINS | CODE | EV (113947, DCM, "Detector Type") | 1 | U |  | DCID 10030 “Detector Types”
19 | > | CONTAINS | NUM | EV (113731, DCM, "Total Number of Radiographic Frames") | 1 | U |  | UNITS = EV (1, UCUM, "no units")
20 | > | CONTAINS | CONTAINER | EV (130502, DCM, "Reference Point Dosimetry") | 1 | U |  |
21 | >> | CONTAINS | TEXT | EV (113780, DCM, "Reference Point Definition") | 1 | MC | XOR Row 22 |
22 | >> | CONTAINS | CODE | EV (113780, DCM, "Reference Point Definition") | 1 | MC | XOR Row 21 | DCID 10025 “Radiation Dose Reference Points”
23 | >> | CONTAINS | NUM | EV (113725, DCM, "Dose (RP) Total") | 1 | U |  | UNITS = EV (Gy, UCUM, "Gy")
24 | >> | CONTAINS | NUM | EV (113728, DCM, "FluoroDose (RP) Total") | 1 | U |  | UNITS = EV (Gy, UCUM, "Gy")
25 | >> | CONTAINS | NUM | EV (113729, DCM, "Acquisition Dose (RP) Total") | 1 | U |  | UNITS = EV (Gy, UCUM, "Gy")
26 | >> | CONTAINS | NUM | EV (113737, DCM, "Distance Source to Reference Point") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
27 | > | CONTAINS | NUM | EV (113812, DCM, "Total Number of Irradiation Events") | 1 | U |  | UNITS = EV ({events}, UCUM, "events")
28 | > | CONTAINS | TEXT | EV (121106, DCM, "Comment") | 1 | U |  |

Content Item Descriptions

Row 2 | Identification the X-Ray source. This designation shall not change for a given source throughout the entire RDSR. Summary-level values that may traditionally include multiple sources, e.g., Dose Area Product Total from planes A and B of a biplane system, could be described by an instance of this template where the Identification of X-Ray Source indicates multiple sources, e.g., "A and B." Summary-level values that are not traditionally described across multiple sources, e.g., Dose (RP) Total on a biplane system, should not accumulate these values across both sources.
Row 5 | Date that the calibration of the equipment's dose indicators was performed.
Row 6 | Typically, a value provided by the medical physicist. The recorded dose or dose area product values in this report can be multiplied by this factor to obtain estimated real-world values. ### Note Note: It is important that this value must not be applied to the measured values before storing them in the report.
Row 7 | Value range from 0 to 100 percent. Uncertainty of the 'actual' value expressed as +/- of the mean.
Row 8 | Identifies Individual or organization responsible for calibration.
Row 9 | Describes calibration protocol according to equipment standards or local guidelines.
Row 10 | The device that produced the irradiation accumulated in this template, i.e., the X-Ray source. This is not required to be present if the information is the same as that already recorded in TID 1004 “Device Observer Identifying Attributes” encoded via the inclusion of TID 1002 “Observer Context” in TID 10040 Row 5.
Row 11 | The total Dose Area Product for all fluoroscopy and acquisition events for a given X-Ray radiation source.
Row 12 | The fluoroscopy component of the total Dose Area Product.
Row 13 | The acquisition component of the total Dose Area Product.
Row 14 | Total clock time of Fluoroscopy accumulated over the defined scope of accumulation (i.e., the sum of the Irradiation Duration values for accumulated fluoroscopy irradiation events).
Row 15 | Total clock time of acquisitions accumulated over the defined scope of accumulation (i.e., the sum of the Irradiation Duration values for accumulated acquisition irradiation events).
Row 21 | A text definition of the Reference Point (RP) used for RP-related dose values.
Row 22 | A coded definition of the Reference Point (RP) used for RP-related dose values.
Row 23 | Accumulated dose relative to reference point.
Row 24 | The fluoroscopic component of the accumulated dose relative to reference point.
Row 25 | The acquisition component of the accumulated dose relative to reference point.
Row 26 | A single value for calculating reference point dose based on fixed distance.
Row 27 | Total Number of irradiation events.

Prev | Up | Next
Enhanced X-Ray Radiation Dose SR IOD Templates | Home | TID 10042 Irradiation Event Summary Data

DICOM PS3.16 2021b - Content Mapping Resource