DICOM PS3.4 2021b - Service Class Specifications

H.4.4.2 DIMSE Service Group (Current)
Prev | H.4.4 Basic Annotation Box SOP Class | Next

#### H.4.4.2 DIMSE Service Group

The DIMSE Services that are applicable to the IOD are shown below.

Table H.4.4.2-1. DIMSE Service Group Applicable to Basic Annotation Box

DICOM Message Service Element | Usage SCU/SCP
--- | ---
N-SET | U/M

The meaning of the Usage SCU/SCP is described in Section H.2.4.

### Note

There is no N-CREATE because the Instances of the Basic Annotation Box SOP Class are created by the Film Box SOP Instance.

This Section describes the behavior of the DIMSE Services that are specific for this IOD. The general behavior of the DIMSE Services is specified in PS3.7.

##### H.4.4.2.1 N-SET

The N-SET is used to update the Basic Annotation Box SOP Instance.

###### H.4.4.2.1.1 Attributes

The Attributes that may be updated are shown in Table H.4-13.

Table H.4-13. N-SET Attributes

Attribute Name | Tag | Usage SCU/SCP
--- | --- | ---
Annotation position | (2030,0010) | M/M
Text String | (2030,0020) | U/M

The meaning of the Usage SCU/SCP is described in Section H.2.4.

###### H.4.4.2.1.2 Status

There are no specific status codes. See PS3.7 for response status codes.

###### H.4.4.2.1.3 Behavior

The SCU uses the N-SET to request the SCP to update a Basic Annotation Box SOP Instance. The SCU shall only specify the SOP Instance UID of the Basic Annotation Box belonging to the last created Film Box SOP Instance in the N-SET request primitive, and shall specify the list of Attributes for which the Attribute Values are to be set. The SCU may erase the text string by setting a zero length value in the Attribute Text String (2030,0020).

The SCP shall set new values for the specified Attributes of the specified SOP Instance.

The SCP shall return the status code of the requested SOP Instance update. The meaning of success, warning, and failure status codes is defined in Section H.2.5.

Prev | Up | Next
H.4.4 Basic Annotation Box SOP Class | Home | H.4.4.3 SOP Class Definition and UID

DICOM PS3.4 2021b - Service Class Specifications