DICOM PS3.3 2021b - Information Object Definitions

C.8.8.14.10 Compensator Transmission and Thickness Data Direction (Current)
Prev | C.8.8.14 RT Beams Module | Next

##### C.8.8.14.10 Compensator Transmission and Thickness Data Direction

The direction of the rows and columns in Compensator Transmission Data (300A,00EB) and Compensator Thickness Data (300A,00EC) is defined as follows: The direction of rows goes along the positive Xb direction and the direction of the columns does along the negative Yb direction of the IEC X-BEAM LIMITING DEVICE coordinate system. Other interpretations shall be documented in an implementation's conformance statement.

Prev | Up | Next
C.8.8.14.9 Compensator Thickness Data and Source to Compensator Distance | Home | C.8.8.14.11 Block and Compensator Precedence for Dosimetric Calculations

DICOM PS3.3 2021b - Information Object Definitions