DICOM PS3.3 2021b - Information Object Definitions

A.7.4 US Multi-frame Image IOD Module Table (Current)
Prev | A.7 Ultrasound Multi-frame Image IOD | Next

### A.7.4 US Multi-frame Image IOD Module Table

Table A.7-1 specifies the Modules of the US Multi-frame Image IOD.

Table A.7-1. US Multi-frame Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | U
Synchronization | C.7.4.2 | C - Required if Modality (0008,0060) = IVUS. May be present otherwise.
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Contrast/Bolus | C.7.6.4 | C - Required if contrast media was used in this image.
Cine | C.7.6.5 | M
Multi-frame | C.7.6.6 | M
Frame Pointers | C.7.6.9 | U
Palette Color Lookup Table | C.7.9 | C - Required if Photometric Interpretation (0028,0004) has a value of PALETTE COLOR
Device | C.7.6.12 | U
Specimen | C.7.6.22 | U
US Region Calibration | C.8.5.5 | U
US Image | C.8.5.6 | M
Overlay Plane | C.9.2 | U
Multi-frame Overlay | C.9.3 | U
VOI LUT | C.11.2 | U
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

### Note

The US Frame of Reference Module was previously included in this IOD, but has been retired. See PS3.3-2003.

#### A.7.4.1 Mutually Exclusive IEs

### Note

A Curve IE was previously included in this IOD that was mutually exclusive with the Image IE, but has been retired. See PS3.3-2004.

Prev | Up | Next
A.7.3 US Image IOD Module Table (Retired) | Home | A.7.4.2 US Image IOD Content Constraints

DICOM PS3.3 2021b - Information Object Definitions