DICOM PS3.16 2021b - Content Mapping Resource

TID 10014 Scanning Length (Current)
Prev | CT Radiation Dose SR IOD Templates | Next

### TID 10014 Scanning Length

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 10014. Scanning Length

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | NUM | EV (113825, DCM, "Scanning Length") | 1 | M |  | UNITS = EV (mm, UCUM, "mm")
2 |  |  | NUM | EV (113893, DCM, "Length of Reconstructable Volume") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
3 |  |  | NUM | EV (113899, DCM, "Exposed Range") | 1 | UC | IFF TID 10013 “CT Irradiation Event Data” row 4 CT Acquisition Type equals (116152004, SCT, "Spiral Acquisition") | UNITS = EV (mm, UCUM, "mm")
4 |  |  | NUM | EV (113895, DCM, "Top Z Location of Reconstructable Volume") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
5 |  |  | NUM | EV (113896, DCM, "Bottom Z Location of Reconstructable Volume") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
6 |  |  | NUM | EV (113897, DCM, "Top Z Location of Scanning Length") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
7 |  |  | NUM | EV (113898, DCM, "Bottom Z Location of Scanning Length") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
8 |  |  | UIDREF | EV (112227, DCM, "Frame of Reference UID") | 1 | MC | IF any of Rows 4 through 7 or Row 34e of TID 10013 are present. | If present, shall be the same UID as in the images reconstructed from this irradiation event.

Content Item Descriptions

Row 1 | For Spiral scanning, the scanning length is normally the table travel in mm during the tube loading (see Figure A-16). For Sequenced scanning, the scanning length is the table travel between consecutive scans times the number of scans. For Stationary and Free scanning, the scanning length is the nominal width of the total collimation.
Row 2 | The length of the reconstructable volume is the maximum z-range between the outermost edges of the top and bottom slices that can be reconstructed from the acquisition. For Spiral scanning, the length of reconstructable volume is the z-range between the outermost beginning of the first reconstructable slice and the outermost end of the last reconstructable slice (see Figure A-16). For Sequenced scanning, the length of reconstructable volume is the z-range between the outermost beginning of the first slice and the outermost end of the last slice (i.e., including any skip). For Stationary and Free scanning, the length of reconstructable volume is the nominal width of the total collimation.
Row 3 | For Spiral scanning, the exposed range is as defined in IEC 60601-2-44 (Ed. 3) 302.115(b) (see Figure A-16). Exposed range is not defined for other modes of scanning.
Rows 4-5 | The Top and Bottom Z Locations of the Reconstructable Volume are independent of the slice width of any actual reconstructed slices. They are measured from the edges of the volume, and hence are not equal to the Z locations encoded in the images of any actual reconstructed slices, which are recorded as the center of the slice.
Rows 4-7 | These locations are patient (not table or gantry) relative, to allow them to be defined in the Patient Coordinate System and hence related to the Image Position (Patient) in the reconstructed images. They are also defined in terms of the top (towards the patient's head), and bottom (towards the patient's feet) of the corresponding ranges, in order to make them independent of whether the scan starts at the top or the bottom or shuttles back and forth in between (see Figure A-16).

Figure A-16. Spiral Acquisition Parameters

Prev | Up | Next
TID 10013 CT Irradiation Event Data | Home | TID 10015 CT Dose Check Details

DICOM PS3.16 2021b - Content Mapping Resource