DICOM PS3.2 2021b - Conformance

M.4 Networking (Current)
Prev | M Conformance Statement Sample DICOM-RTV Service Consumer (Informative) | Next

## M.4 Networking

### M.4.1 Implementation Model

#### M.4.1.1 Application Data Flow

Figure M.4.1-1. Application Data Flow Diagram

The DICOM-RTV Service Application consumes one or multiple DICOM-RTV compliant Flows, transported in RTP over IP, that is/are provided by one other DICOM-RTV Service Application.

#### M.4.1.2 Functional Definition of AEs

##### M.4.1.2.1 Functional Definition of RTV Service Application

The DICOM-RTV Service is Active when the real-time display feature of the equipment is running and some video and/or audio content is provided.

Prev | Up | Next
M.3.3 Additional Remarks for This Example | Home | M.4.2 AE Specifications

DICOM PS3.2 2021b - Conformance