DICOM PS3.3 2021b - Information Object Definitions

A.34.11.4.7 Current Frame Functional Groups Module (Current)
Prev | A.34.11.4 Real-Time Audio Waveform IOD Content Constraints | Next

##### A.34.11.4.7 Current Frame Functional Groups Module

The Current Frame Functional Groups Module shall be placed in the dynamic part of the RTP Payload.

Table A.34.11-2 specifies the Functional Group Macros included in the Current Frame Functional Groups Module for the Real-Time Audio Waveform IOD.

Table A.34.11-2. Real-Time Audio Waveform Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Time of Frame | C.7.6.16.2.29 | M - shall not be used as a Shared Functional Group

Prev | Up | Next
A.34.11.4.6 Waveform Sample Interpretation | Home | A.34.11.4.8 Time Distribution Protocol

DICOM PS3.3 2021b - Information Object Definitions