DICOM PS3.3 2021b - Information Object Definitions

A.7.4.2.2 Active Image Area Overlays (Current)
Prev | A.7.4.2 US Image IOD Content Constraints | Next

##### A.7.4.2.2 Active Image Area Overlays

The Overlay Plane Module and Multi-Frame Overlay Module may be used to describe the active image area by use of a either a single frame overlay that applies to all image frames, or per-frame overlays. In either case, an Overlay Type (60xx,0040) value of R and an appropriate Overlay Subtype (60xx,0045) value is used. In the case of a single frame overlay that applies to all image frames, the active area specified by such an active image area overlay will be at the same location in every frame of the image as specified in Section C.9.2 Overlay Plane Module.

Prev | Up | Next
A.7.4.2 US Image IOD Content Constraints | Home | A.8 Secondary Capture Image IOD

DICOM PS3.3 2021b - Information Object Definitions