DICOM PS3.3 2021c - Information Object Definitions

A.41.4 Ophthalmic Photography 8 Bit Image IOD Content Constraints (Current)
Prev | A.41 Ophthalmic Photography 8 Bit Image IOD | Next

### A.41.4 Ophthalmic Photography 8 Bit Image IOD Content Constraints

The following constraints on Series and Image Attributes take precedence over the descriptions given in the Module Attribute Tables.

#### A.41.4.1 Bits Allocated, Bits Stored, and High Bit

For Ophthalmic Photography 8 bit images, the Enumerated Value of Bits Allocated (0028,0100) (Image Pixel Module, Section C.7.6.3) shall be 8; the Enumerated Value of Bits Stored (0028,0101) shall be 8; and the Enumerated Value of High Bit (0028,0102) shall be 7.

Prev | Up | Next
A.41.3 Ophthalmic Photography 8 Bit Image IOD Modules | Home | A.41.4.2 Contrast/Bolus Agent Sequence

DICOM PS3.3 2021c - Information Object Definitions