DICOM PS3.3 2021c - Information Object Definitions

A.32.9.4.4 Current Frame Functional Groups (Current)
Prev | A.32.9.4 Real-Time Video Endoscopic Image IOD Content Constraints | Next

##### A.32.9.4.4 Current Frame Functional Groups

The C.7.6.27 Current Frame Functional Groups Module shall be placed in the dynamic part of the RTP Payload.

Table A.32.9-2 specifies the Functional Group Macros included in the Current Frame Functional Groups Module for the Real-Time Video Endoscopic Image IOD.

Table A.32.9-2. Real-Time Video Endoscopic Image Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Time of Frame | C.7.6.16.2.29 | M - shall not be used as a Shared Functional Group
Frame Content | C.7.6.16.2.2 | M - shall not be used as a Shared Functional Group
Frame Usefulness | C.7.6.16.2.27 | U - shall not be used as a Shared Functional Group
Camera Position | C.7.6.16.2.28 | U

Prev | Up | Next
A.32.9.4.3 Anatomic Region Sequence | Home | A.32.9.4.5 Time Distribution Protocol

DICOM PS3.3 2021c - Information Object Definitions