DICOM PS3.4 2021c - Service Class Specifications

CC.2.2.4 Status Codes (Current)
Prev | CC.2.2 Request UPS Cancel (N-ACTION) | Next

#### CC.2.2.4 Status Codes

Table CC.2.2-2 defines the status code values that might be returned in a N-ACTION response. General status code values and fields related to status code values are defined for N-ACTION DIMSE Service in PS3.7.

Table CC.2.2-2. N-ACTION Response Status Values [for Request UPS Cancel]

Service Status | Further Meaning | Status Code
--- | --- | ---
Success | The cancel request is acknowledged | 0000
Warning | The UPS is already in the requested state of CANCELED | B304
Failure | Failed: The UPS is already COMPLETED | C311
Failed: Performer chooses not to cancel | C313
Failed: Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307
Failed: The performer cannot be contacted | C312

Prev | Up | Next
CC.2.2.3 Service Class Provider Behavior | Home | CC.2.3 Subscribe/Unsubscribe to Receive UPS Event Reports (N-ACTION)

DICOM PS3.4 2021c - Service Class Specifications