DICOM PS3.4 2021c - Service Class Specifications

CC.2.3.4 Status Codes (Current)
Prev | CC.2.3 Subscribe/Unsubscribe to Receive UPS Event Reports (N-ACTION) | Next

#### CC.2.3.4 Status Codes

Table CC.2.3-3 defines the status code values that might be returned in a N-ACTION response. General status code values and fields related to status code values are defined for N-ACTION DIMSE Service in PS3.7.

Table CC.2.3-3. N-ACTION Response Status Values [for Subscribe/Unsubscribe to Receive UPS sEvent Reports]

Service Status | Further Meaning | Status Code
--- | --- | ---
Success | The requested change of subscription state was performed | 0000
Warning | Deletion Lock not granted. | B301
Failure | Failed: Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307
Failed: Receiving AE-TITLE is Unknown to this SCP | C308
Failed: Specified action not appropriate for specified instance | C314
Failed: SCP does not support Event Reports | C315

Prev | Up | Next
CC.2.3.3 Service Class Provider Behavior | Home | CC.2.4 Report a Change in UPS Status (N-EVENT-REPORT)

DICOM PS3.4 2021c - Service Class Specifications