DICOM PS3.8 2021c - Network Communication Support for Message Exchange

9.3.2.2.2 Transfer Syntax Sub-Item Structure (Current)
Prev | 9.3.2.2 Presentation Context Item Structure | Next

##### 9.3.2.2.2 Transfer Syntax Sub-Item Structure

The Transfer Syntax Sub-Item shall be made of a sequence of mandatory fixed length fields followed by a variable field. Table 9-15 shows the sequence of the mandatory fields.

Table 9-15. Transfer Syntax Sub-Item Fields

Item bytes | Field name | Description of field
--- | --- | ---
1 | Item-type | 40H
2 | Reserved | This reserved field shall be sent with a value 00H but not tested to this value when received.
3-4 | Item-length | This Item-length shall be the number of bytes from the first byte of the following field to the last byte of the Transfer-syntax-name field(s). It shall be encoded as an unsigned binary numbers
5-xxx | Transfer-syntax-name(s) | This variable field shall contain the Transfer-syntax-name proposed for this presentation context. A valid Transfer-syntax-name shall be encoded as defined in Annex F. For a description of the use of this field see Section 7.1.1.13. Transfer-syntax-names are structured as UIDs as defined in PS3.5 (see Annex B for an overview of this concept). DICOM Transfer-syntax-names are registered in PS3.5.

Prev | Up | Next
9.3.2.2 Presentation Context Item Structure | Home | 9.3.2.3 User Information Item Structure

DICOM PS3.8 2021c - Network Communication Support for Message Exchange