DICOM PS3.3 2021c - Information Object Definitions

A.34.14.4.6 Waveform Sample Interpretation (Current)
Prev | A.34.14.4 Electrooculogram IOD Constraints | Next

##### A.34.14.4.6 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in each Waveform Sequence (0054,0100) Item shall be SS or SL.

Prev | Up | Next
A.34.14.4.5 Channel Source and Channel Source Modifiers | Home | A.34.14.4.7 Waveform Annotation Module

DICOM PS3.3 2021c - Information Object Definitions