DICOM PS3.3 2021c - Information Object Definitions

A.32.11.4.2 Frame of Reference Module (Current)
Prev | A.32.11 Dermoscopic Photography Image IOD | Next

#### A.32.11.4.2 Frame of Reference Module

The Frame of Reference Module may be used if multiple successive images are acquired during a single acquisition. All images in a Series that share the same Frame of Reference UID will be spatially related to each other.

Prev | Up | Next
A.32.11.4 Dermoscopic Photography Image IOD Content Constraints | Home | A.32.11.4.3 Acquisition Context Module

DICOM PS3.3 2021c - Information Object Definitions