DICOM PS3.16 2021c - Content Mapping Resource

CID 9565 Treatment Tolerance Violation Causes (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 9565 Treatment Tolerance Violation Causes

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20200624

UID:

  1.2.840.10008.6.1.1322

Table CID 9565. Treatment Tolerance Violation Causes

Coding Scheme Designator | Code Value | Code Meaning | SNOMED-RT ID | UMLS Concept Unique ID
--- | --- | --- | --- | ---
DCM | 130461 | Inappropriate Patient Orientation |  |
DCM | 130462 | Inappropriate Patient Position |  |
DCM | 130463 | Machine Not Available |  |
DCM | 130464 | Change in Patient Anatomy |  |
DCM | 130465 | Machine Calibration Adjustment |  |
DCM | 130466 | Unavailability of a Beam Modifier |  |
DCM | 130467 | Machine Capability License Expired |  |

Prev | Up | Next
CID 9564 Treatment Session Confirmation Assertions | Home | CID 9566 Clinical Tolerance Violation Types

DICOM PS3.16 2021c - Content Mapping Resource