DICOM PS3.3 2021c - Information Object Definitions

A.34.14.4.4 Sampling Frequency (Current)
Prev | A.34.14.4 Electrooculogram IOD Constraints | Next

##### A.34.14.4.4 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence Item is not constrained.

Prev | Up | Next
A.34.14.4.3 Number of Waveform Channels | Home | A.34.14.4.5 Channel Source and Channel Source Modifiers

DICOM PS3.3 2021c - Information Object Definitions