DICOM PS3.16 2021c - Content Mapping Resource

TID 4003 Mammography CAD Individual Impression/Recommendation (Current)
Prev | Mammography CAD SR IOD Templates | Next

### TID 4003 Mammography CAD Individual Impression/Recommendation

This Template collects an individual impression the mammography CAD device had for a lesion, non-lesion object, or correlation of related objects. The details of the impression and recommendation are expressed in the Mammography CAD Impression/Recommendation Body (see TID 4002 “Mammography CAD Impression/Recommendation Body”). The data from which the details are inferred are expressed in the Composite Features (see TID 4004 “Mammography CAD Composite Feature”) and/or Single Image Findings (see TID 4006 “Mammography CAD Single Image Finding”) of which there may be several.

The sub-tree headed by this Template is illustrated in Figure E.1-3 “Example of Individual Impression/Recommendation Levels of Mammography CAD SR Content Tree” in PS3.17 .

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4003. Mammography CAD Individual Impression/Recommendation

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (111034, DCM, "Individual Impression/ Recommendation") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111056, DCM, "Rendering Intent") | 1 | M |  | DCID 6034 “Intended Use of CAD Output”
3 | > | CONTAINS | INCLUDE | DTID 4002 “Mammography CAD Impression/Recommendation Body” | 1 | U |  |
4 | > | CONTAINS | INCLUDE | DTID 4004 “Mammography CAD Composite Feature” | 1-n | MC | At least one of rows 4, 5 shall be present. |
5 | > | CONTAINS | INCLUDE | DTID 4006 “Mammography CAD Single Image Finding” | 1-n | MC | At least one of rows 4, 5 shall be present. |

Content Item Descriptions

Rendering Intent | This Content Item constrains the SCP receiving the Mammography CAD SR IOD in its use of the contents of this Template and its Target Content Items. Mammography CAD devices may opt to use data marked "Not for Presentation" or "Presentation Optional" as input to subsequent mammography CAD processing steps. Refer to Section O.2 “Structured Reporting Storage SOP Class SCU and SCP Behavior” in PS3.4 .

Prev | Up | Next
TID 4002 Mammography CAD Impression/Recommendation Body | Home | TID 4004 Mammography CAD Composite Feature

DICOM PS3.16 2021c - Content Mapping Resource