DICOM PS3.16 2021c - Content Mapping Resource

TID 10052 Attenuator Position (Current)
Prev | Enhanced X-Ray Radiation Dose SR IOD Templates | Next

### TID 10052 Attenuator Position

This template describes the details of the attenuator positions.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10052. Attenuator Position

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (130528, DCM, "Attenuator Position") | 1 | M |  |
2 | > | CONTAINS | DATETIME | DT (111526, DCM, "DateTime Started") | 1 | M |  |
3 | > | CONTAINS | DATETIME | DT (111527, DCM, "DateTime Ended") | 1 | M |  |
4 | > | CONTAINS | CONTAINER | EV (128472, DCM, "X-Ray Beam Attenuator Model") | 1-n | MC | IF an X-Ray Attenuator is described in TID 10047 AND the position is known |
5 | >> | CONTAINS | TEXT | EV (130527, DCM, "Identification of the Attenuator") | 1 | M |  |
6 | >> | CONTAINS | IMAGE | EV (128470, DCM, "X-Ray Attenuator Model Data") | 1 | MC | XOR Row 7, 8 |
7 | >> | CONTAINS | COMPOSITE | EV (128470, DCM, "X-Ray Attenuator Model Data") | 1 | MC | XOR Row 6, 8 |
8 | >> | CONTAINS | UIDREF | EV (128470, DCM, "X-Ray Attenuator Model Data") | 1 | MC | XOR Row 6, 7 |
9 | >> | CONTAINS | TABLE | EV (130520, DCM, "Transformation Matrix") | 1 | M |  | NCOLUMNS = 4 NROWS= 4 CELL VR = FD

Content Item Descriptions

Row 2 | The DateTime of the beginning of the time period over which the content items are applicable.
Row 3 | The DateTime of the end of the time period over which the content items are applicable.
Row 4 | Provide the model and position of each X-Ray attenuator described in TID 10047, if known.
Row 5 | Each X-Ray attenuator model and position description includes the identification of the X-Ray attenuator, which shall match the identification used in TID 10047.
Row 6, 7, 8 | Reference to a three-dimensional model of the X-Ray attenuator
Row 9 | A 4-by-4 matrix of dimensionless numbers of the form defined in Section C.20.2.1.1 “Frame of Reference Transformation Matrix” in PS3.3 . The matrix describes the rigid transformation matrix (including translation and rotation) that transforms the reference coordinate system for the X-Ray attenuator to the RDSR reference coordinate system. The translation described by this matrix indicates the position and orientation of the X-Ray attenuator within the RDSR reference coordinate system. The RCS for the X-Ray attenuator shall be a right-handed Cartesian coordinate system. If the model data in Row 6, 7, 8 was not originally in a right-handed Cartesian coordinate system, it must transformed prior to inclusion in this template.

Prev | Up | Next
TID 10051 Beam Position | Home | TID 10053 Patient Attenuation Characteristics

DICOM PS3.16 2021c - Content Mapping Resource