DICOM PS3.4 2021c - Service Class Specifications

H.4.3.2 Basic Color Image Box SOP Class (Current)
Prev | H.4.3 Image Box SOP Classes | Next

#### H.4.3.2 Basic Color Image Box SOP Class

##### H.4.3.2.1 IOD Description

The Basic Image Box IOD is an abstraction of the presentation of an image and image related data in the image area of a film. The Basic Image Box IOD describes the presentation parameters and image pixel data that apply to a single image of a sheet of film.

The Basic Color Image Box SOP Instance is created by the SCP at the time the Basic Film Box SOP Instance is created, based on the value of the Basic Film Box Attribute Image Display Format (2010,0010).

The Basic Color Image Box SOP Instance refers to zero or one Image Overlay Box SOP Instance.

Prev | Up | Next
H.4.3 Image Box SOP Classes | Home | H.4.3.2.2 DIMSE Service Group

DICOM PS3.4 2021c - Service Class Specifications