DICOM PS3.3 2021c - Information Object Definitions

A.34.11.4.6 Waveform Sample Interpretation (Current)
Prev | A.34.11.4 Real-Time Audio Waveform IOD Content Constraints | Next

##### A.34.11.4.6 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in each Waveform Sequence Item shall be SB or SS.

Prev | Up | Next
A.34.11.4.5 Channel Source | Home | A.34.11.4.7 Current Frame Functional Groups Module

DICOM PS3.3 2021c - Information Object Definitions