DICOM PS3.17 2021c - Explanatory Information

XXX.3.12.3.5 Render Display Module Recommendations (Current)
Prev | XXX.3.12.3 Encoding Details | Next

##### XXX.3.12.3.5 Render Display Module Recommendations

Table XXX.3.12.3.5-1. Render Display Module Recommendations

Attribute Name | Tag | Comment
Pixel Presentation | (0008,9205) | Set to TRUE_COLOR
Volume Stream Sequence | (0070,1A08) |
Item #1 of Volume Stream Sequence
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Presentation State Classification Component Sequence | (0070,1801) |
>Item #1 of Presentation State Classification Component Sequence
>>RGBA Transfer Function Description | (0070,1A09) | Set to "Liver, semi-opaque"
>>Component Type | (0070,1802) | Set to ONE_TO_RGBA
>>Component Input Sequence | (0070,1803) |
>>> Volumetric Presentation Input Index | (0070,1804) | Set to 1
>>RGB LUT Transfer Function | (0028,140F) | TABLE
>>Alpha LUT Transfer Function | (0028,1410) | TABLE
>>Red, Green, Blue Palette Color Lookup Table Descriptors and Data | Orange tint
>>Alpha Palette Color Lookup Table Descriptor and Data | Semi-transparent across liver H.U.range
>Item #2 of Presentation State Classification Component Sequence
>>RGBA Transfer Function Description | (0070,1A09) | Set to "Tumor mass, solid"
>>Component Type | (0070,1802) | Set to ONE_TO_RGBA
>>Component Input Sequence | (0070,1803) |
>>> Volumetric Presentation Input Index | (0070,1804) | Set to 2
>>RGB LUT Transfer Function | (0028,140F) | TABLE
>>Alpha LUT Transfer Function | (0028,1410) | NONE
>>Red, Green, Blue Palette Color Lookup Table Descriptors and Data | Yellow tints
>Item #3 of Presentation State Classification Component Sequence
>>RGBA Transfer Function Description | (0070,1A09) | Set to "Contrast-enhanced vessels, red"
>>Component Type | (0070,1802) | Set to ONE_TO_RGBA
>>Component Input Sequence | (0070,1803) |
>>> Volumetric Presentation Input Index | (0070,1804) | Set to 3
>>RGB LUT Transfer Function | (0028,140F) | TABLE
>>Alpha LUT Transfer Function | (0028,1410) | NONE
>>Red, Green, Blue Palette Color Lookup Table Descriptors and Data | Red tints
Item #2 of Volume Stream Sequence
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID2
>Presentation State Classification Component Sequence | (0070,1801) |
>Item #1 of Presentation State Classification Component Sequence
>>RGBA Transfer Function Description | (0070,1A09) | Set to "Contrast-enhanced vessels, blue"
>>Component Type | (0070,1802) | Set to ONE_TO_RGBA
>>Component Input Sequence | (0070,1803) |
>>>Volumetric Presentation Input Index | (0070,1804) | Set to 4
>>RGB LUT Transfer Function | (0028,140F) | TABLE
>>Alpha LUT Transfer Function | (0028,1410) | NONE
>>Red, Green, Blue Palette Color Lookup Table Descriptors and Data | Blue tints
>Item #2 of Presentation State Classification Component Sequence
>>RGBA Transfer Function Description | (0070,1A09) | Set to "Contrast-enhanced vessels, orange"
>>Component Type | (0070,1802) | Set to ONE_TO_RGBA
>>Component Input Sequence | (0070,1803) |
>>>Volumetric Presentation Input Index | (0070,1804) | Set to 5
>>RGB LUT Transfer Function | (0028,140F) | TABLE
>>Alpha LUT Transfer Function | (0028,1410) | NONE
>>Red, Green, Blue Palette Color Lookup Table Descriptors and Data | Orange tints
Presentation State Compositor Component Sequence | (0070,1805) |
Item #1
>Weighting Transfer Function Sequence | (0070,1806) | Specify tables that give equal weight to both volumes
ICC Profile | (0028,2000) | Value corresponding to IEC 61966-2-1:1999
Color Space | (0028,2002) | Set to SRGB

Prev | Up | Next
XXX.3.12.3.4 Render Shading Module Recommendations | Home | XXX.4 Uses of Presentation View Description in the Identification Module

DICOM PS3.17 2021c - Explanatory Information